TECHNICAL SPECIFICATION
INDUSTRIAL CONSUMABLES AND SPARE PARTS
	Buyer / organisation
	…

	Subject
	Purchase of Industrial Consumables and Spare Parts

	Specification date
	…

	Document no
	…



1. Scope
This technical specification sets out the technical criteria for the purchase of the industrial consumables and spare parts listed in the table below, with their description, technical properties, unit and quantity.
2. Conformity
Products offered shall conform to the national and/or international standards cited in the table. Where the destination market requires a conformity marking (for example CE marking in the European Union and in Türkiye), that marking and the corresponding declaration of conformity shall be provided. Products subject to national registration — biocidal products and certain chemicals are the usual cases — shall carry the registration required in the country of use; the buyer states which country that is.
3. Brands and models
Technical properties are defined by measurable criteria and do not direct the tender towards any particular brand or model. No brand, model, patent, origin or source is named for any line in the table. Naming a brand locks a quotation to a single source and ends the comparison; in public procurement it is restricted or prohibited in many jurisdictions, Türkiye among them. Where a technical property genuinely cannot be expressed in measurable terms, a reference model may be named only together with the words “or equivalent”, and the criteria by which equivalence will be judged shall be written out. “Or equivalent” on its own defines nothing.
4. Packaging and labelling
Products shall be delivered in their original packaging, unopened and undamaged. The packaging shall legibly show the product name, the manufacturer or importer, the batch or serial number, the date of manufacture and, where applicable, the expiry date. Where instructions for use are required, they shall be supplied in the language the buyer specifies.
5. Shelf life
For products carrying an expiry date, at least 75% of the total shelf life shall remain at the date of delivery. Products not meeting this condition will not be accepted. The buyer may set a different percentage; the figure is what makes the clause enforceable.
6. Safety data sheet
For chemical products, a current safety data sheet shall be supplied with the delivery, in the language and format required in the country of use.
7. Samples
The buyer may request free samples of any line during evaluation. Samples shall be delivered with the quotation or within the period the buyer sets. A line for which a sample was requested and not supplied may be excluded from evaluation.
8. Place and time of delivery
Delivery shall be made to the address or addresses notified by the buyer. Carriage and unloading are the supplier's responsibility unless the agreed delivery term states otherwise. For cross-border orders the delivery term shall be stated as an Incoterms 2020 rule (for example EXW, FCA, CPT or DAP); the rule decides who arranges and pays for carriage and where the supplier's responsibility ends. The delivery period is at most … calendar days from order confirmation. Where there is more than one delivery point, the quantity for each point shall be stated separately.
9. Partial delivery
No partial delivery shall be made without the buyer's approval. Where partial delivery is approved, a separate delivery note shall be issued for each consignment.
10. Inspection and acceptance
Delivered products shall be examined against the criteria in this specification. Lines found not to conform shall be recorded and replaced by the supplier, at the supplier's cost, within at most … calendar days. The inspection criteria are the same figures written in the item table — nothing is checked that was not specified.
11. Warranty
Items in the nature of equipment, tools and appliances shall be warranted against manufacturing defects for at least 2 (two) years from the date of delivery. For warranted faults the replacement or repair period shall be at most … working days. Statutory warranty and conformity periods in the country of use apply in addition and are not reduced by this clause.
12. Liability
The supplier is responsible for damage, loss and delay arising in transport up to the point defined by the agreed delivery term. Losses arising from incorrect, incomplete or non-conforming delivery are for the supplier's account.
13. Price and invoicing
Unit prices shall be quoted exclusive of VAT or sales tax; the applicable rate shall be shown on a separate line. The currency shall be stated on the quotation. The quotation shall remain valid for at least … days; where costs are denominated in a foreign currency, the basis of any exchange-rate adjustment shall be written out. Invoicing shall follow delivery as a single invoice unless agreed otherwise.
14. Item list and technical properties
The table below contains 45 items. Delete the rows your organisation does not need, add the rows it does, and complete the “Quantity” column.
	No
	Item
	Technical properties
	Unit
	Quantity

	1
	Bearing, deep groove ball
	Bore, outside diameter, width and seal type stated
	Each
	

	2
	Bearing, tapered roller
	Bore, outside diameter, width and cup or cone stated
	Each
	

	3
	Plummer block housing
	Shaft diameter, housing type and seal arrangement stated
	Each
	

	4
	V-belt
	Profile and datum length stated
	Each
	

	5
	Timing belt
	Pitch, width and tooth count stated
	Each
	

	6
	Roller chain
	Pitch, simplex or duplex and length in links stated
	Metre
	

	7
	Chain sprocket
	Chain pitch, tooth count and bore stated
	Each
	

	8
	Radial shaft seal
	Shaft diameter, housing bore, width and material stated
	Each
	

	9
	O-ring
	Inside diameter, cord thickness and material stated
	Each
	

	10
	Gasket and gasket sheet
	Material, thickness and temperature range stated
	m²
	

	11
	Gland packing
	Cross-section, material and service medium stated
	kg
	

	12
	Flexible coupling
	Bore sizes, torque rating and element type stated
	Each
	

	13
	Hydraulic hose
	Inside diameter, working pressure and fitting type stated
	Each
	

	14
	Pneumatic tubing and fittings
	Outside diameter, material and thread size stated
	Metre
	

	15
	Air preparation unit (FRL)
	Port size, flow rate and filtration grade stated
	Each
	

	16
	Pneumatic cylinder
	Bore, stroke, mounting and cushioning stated
	Each
	

	17
	Solenoid valve
	Port size, function, coil voltage and medium stated
	Each
	

	18
	Hydraulic oil
	Viscosity grade and specification stated
	Drum
	

	19
	Gear oil
	Viscosity grade and specification stated
	Drum
	

	20
	Grease, multipurpose
	NLGI grade and temperature range stated
	Pail
	

	21
	Grease, high temperature
	NLGI grade and maximum service temperature stated
	Each
	

	22
	Cutting fluid
	Dilution ratio and material suitability stated
	Drum
	

	23
	Air filter, compressor
	Element dimensions and filtration grade stated
	Each
	

	24
	Oil filter
	Element dimensions, thread and filtration grade stated
	Each
	

	25
	Hydraulic filter element
	Dimensions, filtration rating and collapse pressure stated
	Each
	

	26
	Dust filter, bag or cartridge
	Dimensions, media and filtration efficiency stated
	Each
	

	27
	Welding electrode, covered
	Classification, diameter and packing weight stated
	Pack
	

	28
	MIG/MAG welding wire
	Classification, diameter and spool weight stated
	Spool
	

	29
	Welding gas regulator
	Gas type, inlet pressure and flow range stated
	Each
	

	30
	Cutting disc, metal
	Diameter, thickness and bore stated
	Each
	

	31
	Grinding disc
	Diameter, thickness, bore and material stated
	Each
	

	32
	Abrasive belt or disc
	Dimensions and grit size stated
	Each
	

	33
	Drill bit, HSS-Co
	Diameter, cobalt content and point angle stated
	Each
	

	34
	Milling and turning tool with insert
	Holder size, insert geometry and grade stated
	Each
	

	35
	Bolt, nut and washer
	Thread size, length, property class and coating stated
	Each
	

	36
	Anchor and fixing
	Diameter, embedment depth, substrate and load rating stated
	Each
	

	37
	Thermometer and pressure gauge
	Range, dial size, connection and accuracy class stated
	Each
	

	38
	Temperature sensor, RTD or thermocouple
	Type, probe length, sheath diameter and range stated
	Each
	

	39
	Inductive proximity sensor
	Body size, sensing distance, output type and supply stated
	Each
	

	40
	Photoelectric sensor
	Sensing mode, range, output type and housing stated
	Each
	

	41
	Encoder
	Incremental or absolute, resolution, shaft size and output
	Each
	

	42
	Variable frequency drive
	Motor power, supply voltage, IP rating and control mode
	Each
	

	43
	Soft starter
	Motor power, supply voltage and bypass option stated
	Each
	

	44
	Maintenance and penetrating spray
	Volume stated; safety data sheet supplied
	Each
	

	45
	Contact cleaner spray
	Plastic-safe formulation; volume stated
	Each
	



15. Approval
This technical specification consists of … pages and … clauses and has been prepared and signed by those named below.
	Prepared by
	Checked by
	Approved by

	Name: …
	Name: …
	Name: …

	Title: …
	Title: …
	Title: …

	Signature:
	Signature:
	Signature:



This template is a general-purpose example and should be adapted to your organisation's requirements and to the rules that apply where you are buying. Fields left as an ellipsis (…) are completed by the buyer. The governing principle behind it is that technical criteria should secure efficiency and fitness for purpose, should not restrict competition, and should give every bidder an equal opportunity — a requirement written into public procurement law in many countries. Check the legislation in force where you are.
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