TECHNICAL SPECIFICATION
TOOLS AND HARDWARE
	Buyer / organisation
	…

	Subject
	Purchase of Tools and Hardware

	Specification date
	…

	Document no
	…



1. Scope
This technical specification sets out the technical criteria for the purchase of the tools and hardware listed in the table below, with their description, technical properties, unit and quantity.
2. Conformity
Products offered shall conform to the national and/or international standards cited in the table. Where the destination market requires a conformity marking (for example CE marking in the European Union and in Türkiye), that marking and the corresponding declaration of conformity shall be provided. Products subject to national registration — biocidal products and certain chemicals are the usual cases — shall carry the registration required in the country of use; the buyer states which country that is.
3. Brands and models
Technical properties are defined by measurable criteria and do not direct the tender towards any particular brand or model. No brand, model, patent, origin or source is named for any line in the table. Naming a brand locks a quotation to a single source and ends the comparison; in public procurement it is restricted or prohibited in many jurisdictions, Türkiye among them. Where a technical property genuinely cannot be expressed in measurable terms, a reference model may be named only together with the words “or equivalent”, and the criteria by which equivalence will be judged shall be written out. “Or equivalent” on its own defines nothing.
4. Packaging and labelling
Products shall be delivered in their original packaging, unopened and undamaged. The packaging shall legibly show the product name, the manufacturer or importer, the batch or serial number, the date of manufacture and, where applicable, the expiry date. Where instructions for use are required, they shall be supplied in the language the buyer specifies.
5. Shelf life
For products carrying an expiry date, at least 75% of the total shelf life shall remain at the date of delivery. Products not meeting this condition will not be accepted. The buyer may set a different percentage; the figure is what makes the clause enforceable.
6. Safety data sheet
For chemical products, a current safety data sheet shall be supplied with the delivery, in the language and format required in the country of use.
7. Samples
The buyer may request free samples of any line during evaluation. Samples shall be delivered with the quotation or within the period the buyer sets. A line for which a sample was requested and not supplied may be excluded from evaluation.
8. Place and time of delivery
Delivery shall be made to the address or addresses notified by the buyer. Carriage and unloading are the supplier's responsibility unless the agreed delivery term states otherwise. For cross-border orders the delivery term shall be stated as an Incoterms 2020 rule (for example EXW, FCA, CPT or DAP); the rule decides who arranges and pays for carriage and where the supplier's responsibility ends. The delivery period is at most … calendar days from order confirmation. Where there is more than one delivery point, the quantity for each point shall be stated separately.
9. Partial delivery
No partial delivery shall be made without the buyer's approval. Where partial delivery is approved, a separate delivery note shall be issued for each consignment.
10. Inspection and acceptance
Delivered products shall be examined against the criteria in this specification. Lines found not to conform shall be recorded and replaced by the supplier, at the supplier's cost, within at most … calendar days. The inspection criteria are the same figures written in the item table — nothing is checked that was not specified.
11. Warranty
Items in the nature of equipment, tools and appliances shall be warranted against manufacturing defects for at least 2 (two) years from the date of delivery. For warranted faults the replacement or repair period shall be at most … working days. Statutory warranty and conformity periods in the country of use apply in addition and are not reduced by this clause.
12. Liability
The supplier is responsible for damage, loss and delay arising in transport up to the point defined by the agreed delivery term. Losses arising from incorrect, incomplete or non-conforming delivery are for the supplier's account.
13. Price and invoicing
Unit prices shall be quoted exclusive of VAT or sales tax; the applicable rate shall be shown on a separate line. The currency shall be stated on the quotation. The quotation shall remain valid for at least … days; where costs are denominated in a foreign currency, the basis of any exchange-rate adjustment shall be written out. Invoicing shall follow delivery as a single invoice unless agreed otherwise.
14. Item list and technical properties
The table below contains 45 items. Delete the rows your organisation does not need, add the rows it does, and complete the “Quantity” column.
	No
	Item
	Technical properties
	Unit
	Quantity

	1
	Combination spanner set
	Size range in mm and piece count stated
	Set
	

	2
	Socket set
	Drive size, socket range and piece count stated
	Set
	

	3
	Torque wrench
	Torque range in Nm, drive size and accuracy class
	Each
	

	4
	Hex key set
	Size range and ball-end option stated
	Set
	

	5
	Hexalobular key set
	Size range and piece count stated
	Set
	

	6
	Adjustable wrench
	Overall length and jaw capacity stated
	Each
	

	7
	Pipe wrench
	Length and pipe capacity stated
	Each
	

	8
	Combination pliers
	Length and insulation rating if required
	Each
	

	9
	Long nose pliers
	Length and tip shape stated
	Each
	

	10
	Diagonal cutting pliers
	Length and maximum cutting capacity stated
	Each
	

	11
	Screwdriver set, slotted and cross
	Tip sizes and piece count stated
	Set
	

	12
	Screwdriver set, insulated
	1000 V insulated, individually tested
	Set
	

	13
	Hammer
	Head weight and handle material stated
	Each
	

	14
	Sledgehammer
	Head weight and handle length stated
	Each
	

	15
	Tape measure
	Length, blade width and accuracy class stated
	Each
	

	16
	Digital caliper
	Measuring range, resolution and accuracy stated
	Each
	

	17
	Spirit level
	Length and accuracy in mm/m stated
	Each
	

	18
	Try square
	Blade length and material stated
	Each
	

	19
	Hacksaw and blades
	Frame length and blade teeth per inch stated
	Set
	

	20
	Utility knife and spare blades
	Blade width and blades per pack stated
	Set
	

	21
	File set
	Cut grade, shapes and piece count stated
	Set
	

	22
	Drill bit set, HSS
	Diameter range and coating stated
	Set
	

	23
	Drill bit set, SDS-plus
	Diameter and working length range stated
	Set
	

	24
	Tap and die set
	Thread range and piece count stated
	Set
	

	25
	Impact drill
	Power in W, chuck capacity and speed range stated
	Each
	

	26
	Cordless drill driver
	Battery voltage and capacity, torque settings, chuck type
	Each
	

	27
	Angle grinder
	Disc diameter, power in W and guard type stated
	Each
	

	28
	Cutting disc
	Diameter, thickness, bore and material stated
	Pack
	

	29
	Grinding disc
	Diameter, thickness, bore and material stated
	Each
	

	30
	Heat gun
	Power in W and temperature range stated
	Each
	

	31
	Caulking gun
	Cartridge size and thrust ratio stated
	Each
	

	32
	Bolt, nut and washer set
	Thread sizes, property class and coating stated
	Set
	

	33
	Wall plug set
	Diameter range, substrate suitability and piece count
	Set
	

	34
	Screw set, wood and sheet metal
	Sizes, head type and coating stated
	Set
	

	35
	Hose clamp
	Clamping range and material stated
	Each
	

	36
	Insulating tape
	Width, length and temperature rating stated
	Each
	

	37
	PTFE thread seal tape
	Width, thickness and length stated
	Each
	

	38
	Penetrating lubricant spray
	Volume stated; safety data sheet supplied
	Each
	

	39
	Grease
	NLGI grade, base type and temperature range stated
	Each
	

	40
	Silicone sealant, clear
	Cartridge volume and cure type stated
	Each
	

	41
	Tool bag
	Dimensions, pocket count and base type stated
	Each
	

	42
	Tool cabinet or trolley
	Drawer count, load per drawer and lock stated
	Each
	

	43
	Inspection lamp
	Light output, cable length and IP rating stated
	Each
	

	44
	Extension cable reel
	Cable length, cross-section, socket count and thermal cut-out
	Each
	

	45
	Step ladder, A-frame
	Working height, step count and load rating stated
	Each
	



15. Approval
This technical specification consists of … pages and … clauses and has been prepared and signed by those named below.
	Prepared by
	Checked by
	Approved by

	Name: …
	Name: …
	Name: …

	Title: …
	Title: …
	Title: …

	Signature:
	Signature:
	Signature:



This template is a general-purpose example and should be adapted to your organisation's requirements and to the rules that apply where you are buying. Fields left as an ellipsis (…) are completed by the buyer. The governing principle behind it is that technical criteria should secure efficiency and fitness for purpose, should not restrict competition, and should give every bidder an equal opportunity — a requirement written into public procurement law in many countries. Check the legislation in force where you are.
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