TECHNICAL SPECIFICATION
PERSONAL PROTECTIVE EQUIPMENT (PPE)
	Buyer / organisation
	…

	Subject
	Purchase of Personal Protective Equipment (PPE)

	Specification date
	…

	Document no
	…



1. Scope
This technical specification sets out the technical criteria for the purchase of the personal protective equipment (ppe) listed in the table below, with their description, technical properties, unit and quantity.
2. Conformity
Products offered shall conform to the national and/or international standards cited in the table. Where the destination market requires a conformity marking (for example CE marking in the European Union and in Türkiye), that marking and the corresponding declaration of conformity shall be provided. Products subject to national registration — biocidal products and certain chemicals are the usual cases — shall carry the registration required in the country of use; the buyer states which country that is.
3. Brands and models
Technical properties are defined by measurable criteria and do not direct the tender towards any particular brand or model. No brand, model, patent, origin or source is named for any line in the table. Naming a brand locks a quotation to a single source and ends the comparison; in public procurement it is restricted or prohibited in many jurisdictions, Türkiye among them. Where a technical property genuinely cannot be expressed in measurable terms, a reference model may be named only together with the words “or equivalent”, and the criteria by which equivalence will be judged shall be written out. “Or equivalent” on its own defines nothing.
4. Packaging and labelling
Products shall be delivered in their original packaging, unopened and undamaged. The packaging shall legibly show the product name, the manufacturer or importer, the batch or serial number, the date of manufacture and, where applicable, the expiry date. Where instructions for use are required, they shall be supplied in the language the buyer specifies.
5. Shelf life
For products carrying an expiry date, at least 75% of the total shelf life shall remain at the date of delivery. Products not meeting this condition will not be accepted. The buyer may set a different percentage; the figure is what makes the clause enforceable.
6. Safety data sheet
For chemical products, a current safety data sheet shall be supplied with the delivery, in the language and format required in the country of use.
7. Samples
The buyer may request free samples of any line during evaluation. Samples shall be delivered with the quotation or within the period the buyer sets. A line for which a sample was requested and not supplied may be excluded from evaluation.
8. Place and time of delivery
Delivery shall be made to the address or addresses notified by the buyer. Carriage and unloading are the supplier's responsibility unless the agreed delivery term states otherwise. For cross-border orders the delivery term shall be stated as an Incoterms 2020 rule (for example EXW, FCA, CPT or DAP); the rule decides who arranges and pays for carriage and where the supplier's responsibility ends. The delivery period is at most … calendar days from order confirmation. Where there is more than one delivery point, the quantity for each point shall be stated separately.
9. Partial delivery
No partial delivery shall be made without the buyer's approval. Where partial delivery is approved, a separate delivery note shall be issued for each consignment.
10. Inspection and acceptance
Delivered products shall be examined against the criteria in this specification. Lines found not to conform shall be recorded and replaced by the supplier, at the supplier's cost, within at most … calendar days. The inspection criteria are the same figures written in the item table — nothing is checked that was not specified.
11. Warranty
Items in the nature of equipment, tools and appliances shall be warranted against manufacturing defects for at least 2 (two) years from the date of delivery. For warranted faults the replacement or repair period shall be at most … working days. Statutory warranty and conformity periods in the country of use apply in addition and are not reduced by this clause.
12. Liability
The supplier is responsible for damage, loss and delay arising in transport up to the point defined by the agreed delivery term. Losses arising from incorrect, incomplete or non-conforming delivery are for the supplier's account.
13. Price and invoicing
Unit prices shall be quoted exclusive of VAT or sales tax; the applicable rate shall be shown on a separate line. The currency shall be stated on the quotation. The quotation shall remain valid for at least … days; where costs are denominated in a foreign currency, the basis of any exchange-rate adjustment shall be written out. Invoicing shall follow delivery as a single invoice unless agreed otherwise.
14. Item list and technical properties
The table below contains 31 items. Delete the rows your organisation does not need, add the rows it does, and complete the “Quantity” column.
	No
	Item
	Technical properties
	Unit
	Quantity

	1
	Safety helmet
	Conforms to EN 397; ventilation and chin strap options stated
	Each
	

	2
	Safety helmet, electrical work
	Electrically insulating class stated; no ventilation holes
	Each
	

	3
	Safety spectacles
	Optical and impact class stated; anti-fog coating option
	Each
	

	4
	Safety goggles
	Sealed frame; impact class and ventilation type stated
	Each
	

	5
	Face shield
	Visor material, impact class and headgear type stated
	Each
	

	6
	Ear plugs
	Attenuation value stated; corded and uncorded options
	Box
	

	7
	Ear defenders, headband
	Attenuation value and helmet-mount option stated
	Each
	

	8
	Disposable respirator, FFP2
	With or without exhalation valve; pack count stated
	Box
	

	9
	Disposable respirator, FFP3
	With or without exhalation valve; pack count stated
	Box
	

	10
	Half mask respirator with filters
	Body to EN 140 plus filters to EN 14387; type and class set by exposure measurement — A2 for solvent work, A2B2E2K2 for mixed gases, combined with P3 where dust or aerosol is present. Connection family stated (EN 148-1 standard thread or proprietary bayonet)
	Set
	

	11
	Spare gas filters (pair)
	To EN 14387 and matching the connection family of the offered mask body; type and class set by exposure measurement (e.g. A2, A2B2E2K2, A2-P3). Type, class, colour band, end of shelf life and manufacturer marked; supplied in unopened packaging
	Pair
	

	12
	Work glove, mechanical protection
	Conforms to EN 388; performance levels and size range stated
	Pair
	

	13
	Work glove, cut resistant
	EN 388 cut level stated; coating type and size range
	Pair
	

	14
	Work glove, heat resistant
	Performance levels and cuff length stated
	Pair
	

	15
	Chemical protective glove
	Material, thickness and breakthrough data required
	Pair
	

	16
	Electrically insulating glove
	Class and test voltage stated; test date required
	Pair
	

	17
	Safety shoe, S1P / S1PL / S1PS
	To EN ISO 20345; toe cap, antistatic, energy absorbing heel and penetration resistance. State all three codes to leave the insert material open (P steel, PL non-metal 4.5 mm, PS non-metal 3.0 mm); naming only one is a deliberate narrowing
	Pair
	

	18
	Safety shoe, S3 / S3L / S3S
	To EN ISO 20345; water resistant upper, penetration resistance and cleated outsole. State all three codes to leave the insert material open — S3S alone excludes steel inserts
	Pair
	

	19
	Safety boot, S5 / S5L / S5S
	Moulded PVC or polyurethane to EN ISO 20345; toe cap, penetration resistance, cleated outsole and antistatic properties. State all three codes to leave the insert material open
	Pair
	

	20
	High visibility vest
	Class and colour stated; tape configuration
	Each
	

	21
	Work coverall
	Fabric composition and g/m² stated; size range
	Each
	

	22
	Welding clothing
	Flame retardant fabric; performance levels stated
	Each
	

	23
	Rainwear set
	Waterproof rating in mm and seam sealing stated
	Set
	

	24
	Full body harness
	Attachment points, size range and inspection record
	Each
	

	25
	Shock absorbing lanyard
	Length, connector type and energy absorber stated
	Each
	

	26
	Retractable fall arrester
	Working length, connector type and inspection interval
	Each
	

	27
	Lifeline and rope grab
	Rope diameter, length and compatible grab stated
	Set
	

	28
	First aid cabinet, wall mounted
	Contents list matched to workplace size
	Each
	

	29
	First aid kit, portable
	Contents list and carrying case type stated
	Each
	

	30
	Eyewash or emergency shower
	Portable bottle or plumbed unit; flow rate stated
	Each
	

	31
	Safety sign set
	Sign size, material and pictogram list stated
	Set
	



15. Approval
This technical specification consists of … pages and … clauses and has been prepared and signed by those named below.
	Prepared by
	Checked by
	Approved by

	Name: …
	Name: …
	Name: …

	Title: …
	Title: …
	Title: …

	Signature:
	Signature:
	Signature:



This template is a general-purpose example and should be adapted to your organisation's requirements and to the rules that apply where you are buying. Fields left as an ellipsis (…) are completed by the buyer. The governing principle behind it is that technical criteria should secure efficiency and fitness for purpose, should not restrict competition, and should give every bidder an equal opportunity — a requirement written into public procurement law in many countries. Check the legislation in force where you are.
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