TECHNICAL SPECIFICATION
CARPET, FLOORING AND ACOUSTIC MATERIALS
	Buyer / organisation
	…

	Subject
	Purchase of Carpet, Flooring and Acoustic Materials

	Specification date
	…

	Document no
	…



1. Scope
This technical specification sets out the technical criteria for the purchase of the carpet, flooring and acoustic materials listed in the table below, with their description, technical properties, unit and quantity.
2. Conformity
Products offered shall conform to the national and/or international standards cited in the table. Where the destination market requires a conformity marking (for example CE marking in the European Union and in Türkiye), that marking and the corresponding declaration of conformity shall be provided. Products subject to national registration — biocidal products and certain chemicals are the usual cases — shall carry the registration required in the country of use; the buyer states which country that is.
3. Brands and models
Technical properties are defined by measurable criteria and do not direct the tender towards any particular brand or model. No brand, model, patent, origin or source is named for any line in the table. Naming a brand locks a quotation to a single source and ends the comparison; in public procurement it is restricted or prohibited in many jurisdictions, Türkiye among them. Where a technical property genuinely cannot be expressed in measurable terms, a reference model may be named only together with the words “or equivalent”, and the criteria by which equivalence will be judged shall be written out. “Or equivalent” on its own defines nothing.
4. Packaging and labelling
Products shall be delivered in their original packaging, unopened and undamaged. The packaging shall legibly show the product name, the manufacturer or importer, the batch or serial number, the date of manufacture and, where applicable, the expiry date. Where instructions for use are required, they shall be supplied in the language the buyer specifies.
5. Shelf life
For products carrying an expiry date, at least 75% of the total shelf life shall remain at the date of delivery. Products not meeting this condition will not be accepted. The buyer may set a different percentage; the figure is what makes the clause enforceable.
6. Safety data sheet
For chemical products, a current safety data sheet shall be supplied with the delivery, in the language and format required in the country of use.
7. Samples
The buyer may request free samples of any line during evaluation. Samples shall be delivered with the quotation or within the period the buyer sets. A line for which a sample was requested and not supplied may be excluded from evaluation.
8. Place and time of delivery
Delivery shall be made to the address or addresses notified by the buyer. Carriage and unloading are the supplier's responsibility unless the agreed delivery term states otherwise. For cross-border orders the delivery term shall be stated as an Incoterms 2020 rule (for example EXW, FCA, CPT or DAP); the rule decides who arranges and pays for carriage and where the supplier's responsibility ends. The delivery period is at most … calendar days from order confirmation. Where there is more than one delivery point, the quantity for each point shall be stated separately.
9. Partial delivery
No partial delivery shall be made without the buyer's approval. Where partial delivery is approved, a separate delivery note shall be issued for each consignment.
10. Inspection and acceptance
Delivered products shall be examined against the criteria in this specification. Lines found not to conform shall be recorded and replaced by the supplier, at the supplier's cost, within at most … calendar days. The inspection criteria are the same figures written in the item table — nothing is checked that was not specified.
11. Warranty
Items in the nature of equipment, tools and appliances shall be warranted against manufacturing defects for at least 2 (two) years from the date of delivery. For warranted faults the replacement or repair period shall be at most … working days. Statutory warranty and conformity periods in the country of use apply in addition and are not reduced by this clause.
12. Liability
The supplier is responsible for damage, loss and delay arising in transport up to the point defined by the agreed delivery term. Losses arising from incorrect, incomplete or non-conforming delivery are for the supplier's account.
13. Price and invoicing
Unit prices shall be quoted exclusive of VAT or sales tax; the applicable rate shall be shown on a separate line. The currency shall be stated on the quotation. The quotation shall remain valid for at least … days; where costs are denominated in a foreign currency, the basis of any exchange-rate adjustment shall be written out. Invoicing shall follow delivery as a single invoice unless agreed otherwise.
14. Item list and technical properties
The table below contains 24 items. Delete the rows your organisation does not need, add the rows it does, and complete the “Quantity” column.
	No
	Item
	Technical properties
	Unit
	Quantity

	1
	Carpet tile
	500 × 500 mm; ISO 10874 use class, pile weight and backing stated
	m²
	

	2
	Broadloom carpet
	4 m width; ISO 10874 use class and pile weight stated
	m²
	

	3
	LVT vinyl tile
	Thickness, wear layer in microns and use class stated
	m²
	

	4
	Homogeneous vinyl sheet
	Thickness, use class and welding rod priced separately
	m²
	

	5
	Laminate flooring
	Thickness, use class, locking system and underlay separate
	m²
	

	6
	Epoxy floor coating
	Coats, dry film thickness and application temperature range
	m²
	

	7
	Floor primer and screed repair mortar
	Absorbency, layer thickness and cure time stated
	kg
	

	8
	Flooring adhesive
	Type matched to covering; coverage in m²/kg stated
	kg
	

	9
	Skirting and edge profile
	Height, material and fixing method stated; priced per metre
	m
	

	10
	Transition and level change profile
	Width, height difference and finish stated
	m
	

	11
	Stair nosing, anti-slip
	Width, insert type and fixing method stated
	m
	

	12
	Raised access floor panel
	Panel size, load class, finish and pedestal height stated
	m²
	

	13
	Entrance matting system
	Zone type, recessed or surface, dimensions and drainage
	m²
	

	14
	Anti-slip tape
	Width, grit grade, colour and roll length stated
	Roll
	

	15
	Acoustic wall panel
	Panel size, thickness, fabric finish and fire reaction class
	m²
	

	16
	Acoustic ceiling tile
	Tile size, thickness, edge detail and fire reaction class
	m²
	

	17
	Acoustic baffle and ceiling raft
	Dimensions, suspension kit and fire reaction class stated
	Each
	

	18
	Acoustic desk and floor screen
	Dimensions, core material and mounting method stated
	Each
	

	19
	Impact sound insulation underlay
	Thickness and impact sound reduction data required
	m²
	

	20
	Suspended ceiling grid
	Grid module, profile type and hanger spacing stated
	m²
	

	21
	Carpet cleaning and maintenance chemicals
	For extraction or encapsulation; dilution ratio stated
	Drum
	

	22
	Floor polish and sealer
	Coats, coverage and slip resistance information stated
	Drum
	

	23
	Flooring installation and removal service
	Scope: lift, level, prime, lay, skirting and waste removal
	Service
	

	24
	Floor survey and measurement
	Area take-off, moisture check and levelness assessment
	Service
	



15. Approval
This technical specification consists of … pages and … clauses and has been prepared and signed by those named below.
	Prepared by
	Checked by
	Approved by

	Name: …
	Name: …
	Name: …

	Title: …
	Title: …
	Title: …

	Signature:
	Signature:
	Signature:



This template is a general-purpose example and should be adapted to your organisation's requirements and to the rules that apply where you are buying. Fields left as an ellipsis (…) are completed by the buyer. The governing principle behind it is that technical criteria should secure efficiency and fitness for purpose, should not restrict competition, and should give every bidder an equal opportunity — a requirement written into public procurement law in many countries. Check the legislation in force where you are.
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