TECHNICAL SPECIFICATION
PAINT AND PAINTING ANCILLARIES
	Buyer / organisation
	…

	Subject
	Purchase of Paint and Painting Ancillaries

	Specification date
	…

	Document no
	…



1. Scope
This technical specification sets out the technical criteria for the purchase of the paint and painting ancillaries listed in the table below, with their description, technical properties, unit and quantity.
2. Conformity
Products offered shall conform to the national and/or international standards cited in the table. Where the destination market requires a conformity marking (for example CE marking in the European Union and in Türkiye), that marking and the corresponding declaration of conformity shall be provided. Products subject to national registration — biocidal products and certain chemicals are the usual cases — shall carry the registration required in the country of use; the buyer states which country that is.
3. Brands and models
Technical properties are defined by measurable criteria and do not direct the tender towards any particular brand or model. No brand, model, patent, origin or source is named for any line in the table. Naming a brand locks a quotation to a single source and ends the comparison; in public procurement it is restricted or prohibited in many jurisdictions, Türkiye among them. Where a technical property genuinely cannot be expressed in measurable terms, a reference model may be named only together with the words “or equivalent”, and the criteria by which equivalence will be judged shall be written out. “Or equivalent” on its own defines nothing.
4. Packaging and labelling
Products shall be delivered in their original packaging, unopened and undamaged. The packaging shall legibly show the product name, the manufacturer or importer, the batch or serial number, the date of manufacture and, where applicable, the expiry date. Where instructions for use are required, they shall be supplied in the language the buyer specifies.
5. Shelf life
For products carrying an expiry date, at least 75% of the total shelf life shall remain at the date of delivery. Products not meeting this condition will not be accepted. The buyer may set a different percentage; the figure is what makes the clause enforceable.
6. Safety data sheet
For chemical products, a current safety data sheet shall be supplied with the delivery, in the language and format required in the country of use.
7. Samples
The buyer may request free samples of any line during evaluation. Samples shall be delivered with the quotation or within the period the buyer sets. A line for which a sample was requested and not supplied may be excluded from evaluation.
8. Place and time of delivery
Delivery shall be made to the address or addresses notified by the buyer. Carriage and unloading are the supplier's responsibility unless the agreed delivery term states otherwise. For cross-border orders the delivery term shall be stated as an Incoterms 2020 rule (for example EXW, FCA, CPT or DAP); the rule decides who arranges and pays for carriage and where the supplier's responsibility ends. The delivery period is at most … calendar days from order confirmation. Where there is more than one delivery point, the quantity for each point shall be stated separately.
9. Partial delivery
No partial delivery shall be made without the buyer's approval. Where partial delivery is approved, a separate delivery note shall be issued for each consignment.
10. Inspection and acceptance
Delivered products shall be examined against the criteria in this specification. Lines found not to conform shall be recorded and replaced by the supplier, at the supplier's cost, within at most … calendar days. The inspection criteria are the same figures written in the item table — nothing is checked that was not specified.
11. Warranty
Items in the nature of equipment, tools and appliances shall be warranted against manufacturing defects for at least 2 (two) years from the date of delivery. For warranted faults the replacement or repair period shall be at most … working days. Statutory warranty and conformity periods in the country of use apply in addition and are not reduced by this clause.
12. Liability
The supplier is responsible for damage, loss and delay arising in transport up to the point defined by the agreed delivery term. Losses arising from incorrect, incomplete or non-conforming delivery are for the supplier's account.
13. Price and invoicing
Unit prices shall be quoted exclusive of VAT or sales tax; the applicable rate shall be shown on a separate line. The currency shall be stated on the quotation. The quotation shall remain valid for at least … days; where costs are denominated in a foreign currency, the basis of any exchange-rate adjustment shall be written out. Invoicing shall follow delivery as a single invoice unless agreed otherwise.
14. Item list and technical properties
The table below contains 31 items. Delete the rows your organisation does not need, add the rows it does, and complete the “Quantity” column.
	No
	Item
	Technical properties
	Unit
	Quantity

	1
	Interior emulsion paint
	Wet scrub class and spreading rate in m²/L stated
	Pail
	

	2
	Interior satin paint
	Wet scrub class, sheen level and spreading rate stated
	Pail
	

	3
	Ceiling paint
	Matt finish; opacity class and spreading rate stated
	Pail
	

	4
	Exterior acrylic paint
	Water vapour and liquid water transmission classes stated
	Pail
	

	5
	Alkyd gloss paint
	Solvent based; overcoat interval and spreading rate stated
	Box
	

	6
	Primer, interior
	Water based; absorbency regulation and spreading rate
	Pail
	

	7
	Primer, exterior
	Binding primer; spreading rate and overcoat interval
	Pail
	

	8
	Anti-corrosive primer
	For steel; dry film thickness and overcoat interval stated
	Box
	

	9
	Epoxy floor paint
	Two component; coats, dry film thickness and pot life stated
	Set
	

	10
	Road and yard line marking paint
	Drying time and coverage per linear metre stated
	Pail
	

	11
	Heat resistant paint
	Maximum service temperature stated
	Each
	

	12
	Finishing plaster, powder
	Mixing ratio, pot life and layer thickness stated
	Bag
	

	13
	Ready mixed filler
	Layer thickness and drying time stated
	Pail
	

	14
	Joint compound and tape
	For plasterboard joints; tape width stated
	Set
	

	15
	Paint roller, short pile
	Pile height and roller width stated; for smooth surfaces
	Each
	

	16
	Paint roller, medium pile
	Pile height and roller width stated
	Each
	

	17
	Paint roller, long pile
	Pile height and roller width stated; for textured surfaces
	Each
	

	18
	Paint roller, mohair
	Short pile; for gloss and satin finishes
	Each
	

	19
	Roller frame
	Roller width and handle thread stated
	Each
	

	20
	Extension pole, telescopic
	Extended length and thread type stated
	Each
	

	21
	Paint brush, flat
	Width, bristle type and handle material stated
	Each
	

	22
	Radiator brush
	Angled long handle; width stated
	Each
	

	23
	Paint tray
	Roller width compatibility and liner option
	Each
	

	24
	Masking tape
	Width, length and removal time stated
	Each
	

	25
	Protective sheeting
	Micron thickness and sheet size stated
	Each
	

	26
	Floor protection fleece
	Width, length and absorbency stated
	Roll
	

	27
	Abrasive paper, hand
	Grit size and sheet dimensions stated
	Pack
	

	28
	Abrasive disc, hook and loop
	Diameter, grit and hole pattern stated
	Pack
	

	29
	Filling knife and trowel set
	Blade widths and material stated
	Set
	

	30
	Paint mixing paddle
	Shaft diameter and paddle length stated
	Each
	

	31
	Thinner, synthetic
	Safety data sheet supplied; storage requirements apply
	Drum
	



15. Approval
This technical specification consists of … pages and … clauses and has been prepared and signed by those named below.
	Prepared by
	Checked by
	Approved by

	Name: …
	Name: …
	Name: …

	Title: …
	Title: …
	Title: …

	Signature:
	Signature:
	Signature:



This template is a general-purpose example and should be adapted to your organisation's requirements and to the rules that apply where you are buying. Fields left as an ellipsis (…) are completed by the buyer. The governing principle behind it is that technical criteria should secure efficiency and fitness for purpose, should not restrict competition, and should give every bidder an equal opportunity — a requirement written into public procurement law in many countries. Check the legislation in force where you are.
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